Id - Owners / Station Identification:COE: US Army Corps of EngineersJMA: Japanese Meteorological AgencyNOS: National Ocean Service, NOAAPMEL: Pacific Marine Environmental Laboratory, NOAAPTWC: Pacific Tsunami Warning Center, NWSUHSLC: University of Hawaii Sea Level Centerblank: Owners of individually maintained Japanese stations not available at this time.T - Tsunami Visible?:Y: Indicates tsunami signal is evident above noise levels.?: Indicates tsunami signal is questionable, but might be evident with more processing.N: Indicates tsunami signal is not evident above noise levels.Sensors:ADR: Data from a punch paper tape transmitted via satelliteAquatrak: Data from AQUATRAK sensor transmitted via satelliteBPR: Data from PAROSCIENTIFIC sensorDruck: Data from DRUCK Sensor stored on 64K RAM packIMO: Data from IMO Sensor stored on 64K RAM packBUB: Data from BUBBLER gauge transmitted via satelliteENC: DATA from HANDAR ENCODER transmitted via satellitePRS: Data from NOS PRESSURE TRANSDUCER transmitted via satellitePTW: Data from NOS PRIMARY WATER LEVEL transmitted via satelliteblank: not available at this time.ETA - Estimated Time of Arrival:Tsunami arrival time at each station, relative to the main earthquake shock (June 10, 1996 at0404 UTC), estimated by means of a modified PTWC travel time code.Mean:Mean sea level value removed from data records.